


interrupt RasterScene1();
begin
	startirq(@useKernal);
	ProgressTracker();

	closeIRQ();
end;





procedure InitScene1();
begin
	SCREEN_BG_COL:=BLACK;
	SCREEN_FG_COL:=BLACK;
	setbank(VIC_BANK1);
	// Use the 3rd column of the timestamp to specify index of the packed data!
	i:=timeStamps[currentPart*4+2];
	// Enable reading $D000-$DFFF
	enableallram();
	// Decrunch image data to $6000	
	decrunchfromindex(packed_data_addresses,i); 
	// Decrunch color data to $4800
	decrunchfromindex(packed_data_addresses,i+1);
	// Restore memory config
	poke(^$01, 0,keep01);
	// Don't copy color data: Set everything black
	copyimagecolordata(^$4800,1);
	
	// Enable multicolor bitmap image at location $6000
	poke(VIC_DATA_LOC, 0,$18);
	setbitmapmode();
	setmulticolormode();

end;
