# VICE keyboard mapping file
#
# A Keyboard map is read in as patch to the current map.
#
# File format:
# - comment lines start with '#'
# - keyword lines start with '!keyword'
# - normal line has 'keysym/scancode row column shiftflag'
#
# Keywords and their lines are:
# '!CLEAR'               clear whole table
# '!INCLUDE filename'    read file as mapping file
# '!LSHIFT row col'      left shift keyboard row/column
# '!RSHIFT row col'      right shift keyboard row/column
# '!VSHIFT shiftkey'     virtual shift key (RSHIFT or LSHIFT)
# '!SHIFTL shiftkey'     shift lock key (RSHIFT or LSHIFT)
# '!UNDEF keysym'        remove keysym from table
#
# Shiftflag can have the values:
# 0      key is not shifted for this keysym/scancode
# 1      key is shifted for this keysym/scancode
# 2      left shift
# 4      right shift
# 8      key can be shifted or not with this keysym/scancode
# 16     deshift key for this keysym/scancode
# 32     another definition for this keysym/scancode follows
# 64     shift lock
# 256    key is used for an alternative keyboard mapping
#
# Negative row values:
# 'keysym -1 n' joystick keymap A, direction n
# 'keysym -2 n' joystick keymap B, direction n
# 'keysym -3 0' first RESTORE key
# 'keysym -3 1' second RESTORE key
# 'keysym -4 0' 40/80 column key
# 'keysym -4 1' CAPS (ASCII/DIN) key
# 'keysym -5 n' joyport keypad, key n
#
# Joystick direction values:
# 0      Fire
# 1      South/West
# 2      South
# 3      South/East
# 4      West
# 5      East
# 6      North/West
# 7      North
# 8      North/East
#
# Joyport keypad key layout:
# --------------------------
# |  0 |  1 |  2 |  3 |  4 |
# --------------------------
# |  5 |  6 |  7 |  8 |  9 |
# --------------------------
# | 10 | 11 | 12 | 13 | 14 |
# --------------------------
# | 15 | 16 | 17 | 18 | 19 |
# --------------------------
#
# When a bigger spaced key is used,
# it uses the upper left most key value.

# Positional Mapping for Individual Computer's "Keyrah", US Layout, C64, SDL

# This mapping was created specifically for use with "Combian" on the
# Combian, which apparently has a slightly broken keyboard mapping in SDL

# For this mapping to work the keyboard in raspian must be PC-105 (GB)

# this keyboard map applies for the "vice" setting of keyrah (switch down) and
# maps all 64 keys, plus restore, to the respective emulated keys in the 
# emulation. this however leaves no key free to enter the menu - one way to work
# around this is to configure the "enter menu" key to the code which is produced
# by the arrow up key when the switch is in "normal" (middle) position, like:
#
# MenuKey=281                    arrow up for menu (with switch in middle pos.)
#
# in combian you could add this to the sdl-vicerc file, which is located in
# /root/.vice/sdl-vicerc

# C64 keyboard matrix:
#
#       +-----+-----+-----+-----+-----+-----+-----+-----+
#       |Bit 0|Bit 1|Bit 2|Bit 3|Bit 4|Bit 5|Bit 6|Bit 7|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+

!CLEAR
!LSHIFT 1 7
!RSHIFT 6 4
!VSHIFT RSHIFT
!SHIFTL LSHIFT

8   0 0 8               /*    backspace -> Del          */
13  0 1 8               /*       Return -> Return       */
275 0 2 8               /*        Right -> CRSR RIGHT   */
#276 0 2 1               /*         Left -> CRSR LEFT    */
288 0 3 8               /*           F7 -> F7           */
#289 0 3 1               /*           F8 -> F8           */
282 0 4 8               /*           F1 -> F1           */
#283 0 4 1               /*           F2 -> F2           */
284 0 5 8               /*           F3 -> F3           */
#285 0 5 1               /*           F4 -> F4           */
286 0 6 8               /*           F5 -> F5           */
#287 0 6 1               /*           F6 -> F6           */
#273 0 7 1               /*           Up -> CRSR UP      */
274 0 7 8               /*         Down -> CRSR DOWN    */

51  1 0 8               /*            3 -> 3            */
52  1 3 8               /*            4 -> 4            */
304 1 7 2               /*   Left Shift -> Left Shift   */
#301 1 7 64              /*    Caps Lock -> Shift Lock   */

53  2 0 8               /*            5 -> 5            */
54  2 3 8               /*            6 -> 6            */

55  3 0 8               /*            7 -> 7            */
56  3 3 8               /*            8 -> 8            */

57  4 0 8               /*            9 -> 9            */
48  4 3 8               /*            0 -> 0            */

#223 5 0 8               /*     world 63 -> +            */
45  5 0 8               /*            + -> +            */
#180 5 3 8               /*     world 20 -> -            */
61  5 3 8               /*            - -> -            */
46  5 4 8               /*            . -> .            */
#246 5 5 8               /*     world 86 -> :            */
59  5 5 8               /*            : -> :            */
#252 5 6                 /*     world 92 -> @            */
91  5 6 8               /*     world 92 -> @            */
44  5 7 8               /*            , -> ,            */

277 6 0 8               /*        Pound -> Pound        */
#43  6 1 8               /*            * -> *            */
93  6 1 8               /*            * -> *            */
#228 6 2 8               /*     world 68 -> ;            */
39  6 2 8               /*            ; -> ;            */
278 6 3 8               /*         Home -> CLR/HOME     */
303 6 4 4               /*  Right Shift -> Right Shift  */
#35  6 5 8               /*            = -> =           */
92 6 5 8               /*            \ -> =            */
127 6 6 8               /*     Up Arrow -> Up Arrow     */
#45  6 7 8               /*            - -> /            */
47  6 7 8               /*            / -> /            */

49  7 0 8               /*            1 -> 1            */
#94  7 1 8               /*            ^ -> Left Arrow   */
96  7 1 8               /*   Left Arrow -> Left Arrow   */
9   7 2 8               /*         Ctrl -> Ctrl         */
50  7 3 8               /*            2 -> 2            */
32  7 4 8               /*        Space -> Space        */
306 7 5 8               /*          CBM -> CBM          */
27  7 7 8               /*     Run/Stop -> Run/Stop     */

97  1 2 8               /*            A -> A            */
98  3 4 8               /*            B -> B            */
99  2 4 8               /*            C -> C            */
100 2 2 8               /*            D -> D            */
101 1 6 8               /*            E -> E            */
102 2 5 8               /*            F -> F            */
103 3 2 8               /*            G -> G            */
104 3 5 8               /*            H -> H            */
105 4 1 8               /*            I -> I            */
106 4 2 8               /*            J -> J            */
107 4 5 8               /*            K -> K            */
108 5 2 8               /*            L -> L            */
109 4 4 8               /*            M -> M            */
110 4 7 8               /*            N -> N            */
111 4 6 8               /*            O -> O            */
112 5 1 8               /*            P -> P            */
113 7 6 8               /*            Q -> Q            */
114 2 1 8               /*            R -> R            */
115 1 5 8               /*            S -> S            */
116 2 6 8               /*            T -> T            */
117 3 6 8               /*            U -> U            */
118 3 7 8               /*            V -> V            */
119 1 1 8               /*            W -> W            */
120 2 7 8               /*            X -> X            */

121 3 1 8               /*            Y -> Y            */
122 1 4 8               /*            Z -> Z            */

# Restore key
280 -3 0

# joystick keymap A (port 1)
256 -1 0              /*     NumPad 0 -> FIRE         */
265 -1 7              /*     NumPad 9 -> UP           */
259 -1 2              /*     NumPad 3 -> DOWN         */
263 -1 4              /*     NumPad 7 -> LEFT         */
257 -1 5              /*     NumPad 1 -> RIGHT        */

# joystick Keymap B (port 2)
261 -2 0              /*     NumPad 5 -> FIRE         */
264 -2 7              /*     NumPad 8 -> UP           */
258 -2 2              /*     NumPad 2 -> DOWN         */
260 -2 4              /*     NumPad 4 -> LEFT         */
262 -2 5              /*     NumPad 6 -> RIGHT        */

# Joyport attached keypad key mappings
# note: there are no such keys on the C64 keyboard connected to keyrah
#300 -5 0              /*      NumLock -> keypad x0    */
#263 -5 1              /*     NumPad 7 -> keypad 7     */
#264 -5 2              /*     NumPad 8 -> keypad 8     */
#265 -5 3              /*     NumPad 9 -> keypad 9     */
#267 -5 4              /*     NumPad / -> keypad /     */
#302 -5 5              /*   ScrollLock -> keypad x1    */
#260 -5 6              /*     NumPad 4 -> keypad 4     */
#261 -5 7              /*     NumPad 5 -> keypad 5     */
#262 -5 8              /*     NumPad 6 -> keypad 6     */
#268 -5 9              /*     NumPad * -> keypad *     */
#317 -5 10             /*       SysReq -> keypad x2    */
#257 -5 11             /*     NumPad 1 -> keypad 1     */
#258 -5 12             /*     NumPad 2 -> keypad 2     */
#259 -5 13             /*     NumPad 3 -> keypad 3     */
#269 -5 14             /*     NumPad - -> keypad -     */
#316 -5 15             /*       PrtScr -> keypad x3    */
#256 -5 16             /*     NumPad 0 -> keypad 0     */
#266 -5 17             /*     NumPad , -> keypad .     */
#271 -5 18             /* NumPad Enter -> keypad enter */
#270 -5 19             /*     NumPad + -> keypad +     */
