# VICE keyboard mapping file
#
# A Keyboard map is read in as patch to the current map.
#
# File format:
# - comment lines start with '#'
# - keyword lines start with '!keyword'
# - normal line has 'keysym/scancode row column shiftflag'
#
# Keywords and their lines are:
# '!CLEAR'               clear whole table
# '!INCLUDE filename'    read file as mapping file
# '!LSHIFT row col'      left shift keyboard row/column
# '!RSHIFT row col'      right shift keyboard row/column
# '!VSHIFT shiftkey'     virtual shift key (RSHIFT or LSHIFT)
# '!SHIFTL shiftkey'     shift lock key (RSHIFT or LSHIFT)
# '!LCTRL row col'       left control keyboard row/column
# '!VCTRL ctrlkey'       virtual control key (LCTRL)
# '!LCBM row col'        left CBM keyboard row/column
# '!VCBM cbmkey'         virtual CBM key (LCBM)
# '!UNDEF keysym'        remove keysym from table
#
# Shiftflag can have the values:
# 0      key is not shifted for this keysym/scancode
# 1      key is combined with shift for this keysym/scancode
# 2      key is left shift on emulated machine
# 4      key is right shift on emulated machine
# 8      key can be shifted or not with this keysym/scancode
# 16     deshift key for this keysym/scancode
# 32     another definition for this keysym/scancode follows
# 64     key is shift-lock on emulated machine
# 128    shift modifier required on host
# 256    key is used for an alternative keyboard mapping
# 512    alt-r (alt-gr) modifier required on host
# 1024   ctrl modifier required on host
# 2048   key is combined with cbm for this keysym/scancode
# 4096   key is combined with ctrl for this keysym/scancode
# 8192   key is (left) cbm on emulated machine
# 16384  key is (left) ctrl on emulated machine
#
# to migrate older keymaps and use the CBM and/or CTRL related features:
#
# - define !LCTRL, !VCTRL, !LCBM, !VCBM
# - add 'key is (left) cbm/ctrl on emulated machine' flags to
#   all keys that map to the cbm or ctrl key respectively.
#
# after that the virtual cbm/ctrl flags and requiring host modifiers
# should work as expected. keep an eye on the error messages.
#
# Negative row values:
# 'keysym -1 n' joystick keymap A, direction n
# 'keysym -2 n' joystick keymap B, direction n
# 'keysym -3 0' first RESTORE key
# 'keysym -3 1' second RESTORE key
# 'keysym -4 0' 40/80 column key
# 'keysym -4 1' CAPS (ASCII/DIN) key
# 'keysym -5 n' joyport keypad, key n
#
# Joystick direction values:
# 0      Fire
# 1      South/West
# 2      South
# 3      South/East
# 4      West
# 5      East
# 6      North/West
# 7      North
# 8      North/East
#
# Joyport keypad key layout:
# --------------------------
# |  0 |  1 |  2 |  3 |  4 |
# --------------------------
# |  5 |  6 |  7 |  8 |  9 |
# --------------------------
# | 10 | 11 | 12 | 13 | 14 |
# --------------------------
# | 15 | 16 | 17 | 18 | 19 |
# --------------------------
#
# When a bigger spaced key is used,
# it uses the upper left most key value.

# Positional Mapping, Swedish Layout, C64, X11

# C64 keyboard matrix:
#
#       +-----+-----+-----+-----+-----+-----+-----+-----+
#       |Bit 0|Bit 1|Bit 2|Bit 3|Bit 4|Bit 5|Bit 6|Bit 7|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+

!CLEAR
!LSHIFT 1 7
!RSHIFT 6 4
!VSHIFT RSHIFT
!SHIFTL LSHIFT
!LCBM 7 5
!VCBM LCBM
!LCTRL 7 2
!VCTRL LCTRL

# keys that can't be mapped positionally are:
# (row0) pound (-> </>), clr/home (-> home)
# (row1) arrow up (-> end), restore (-> F12)
# (row2) run/stop (-> escape)
# (row3) commodore (-> control)

# extra keys are:
# clr/home (-> altgr+\)
# ins/del (-> delete)
# ins/del+shift (-> insert)
# arrow up (-> altgr+~)
# arrow up+shift (-> altgr+m)
# f1 (-> page up)
# f7 (-> page down)
# :+shift (-> altgr+[)
# ;+shift (-> altgr+])
# @ (-> altgr+Q)

#####################
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|

# inst/del
BackSpace        0 0 8
# extra: delete -> ins/del
Delete           0 0 8
# extra: insert -> shift+ins/del
Insert           0 0 1
# return
Return           0 1 8
# cursor r/l
Right            0 2 8
Left             0 2 1
# f7
F7               0 3 8
F8               0 3 1
# extra: pagedown -> f7
Page_Down        0 3 8
# f1
F1               0 4 8
F2               0 4 1
# extra: pagedown -> f1
Page_Up          0 4 8
# f3
F3               0 5 8
F4               0 5 1
# f4
F5               0 6 8
F6               0 6 1
# cursor u/d
Up               0 7 1
Down             0 7 8

#####################
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |

# shift+3
numbersign       1 0 8
# shift+4
EuroSign         1 3 8
# left shift
# key is left shift
Shift_L          1 7 2
# shift lock
# key is (left) shift-lock
Caps_Lock        1 7 64

#####################
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |

# shift+5
percent          2 0 8
# shift+6
ampersand        2 3 8

#####################
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |

# shift+7
slash            3 0 8
# shift+8
parenleft        3 3 8

#####################
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |

# shift+9
parenright       4 0 8
# shift+0
equal            4 3 8
#####################
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |

# plus
plus             5 0 8
question         5 0 8
# minus
acute            5 3 8
grave            5 3 8
# dot
period           5 4 8
colon            5 4 1
# colon
odiaeresis       5 5 8
Odiaeresis       5 5 1
# extra: altgr+[ -> :+shift
bracketleft      5 5 1
# @-key
aring            5 6 8
Aring            5 6 1
# extra: altgr+Q -> @
at               5 6 0
# comma
comma            5 7 8
semicolon        5 7 1

#####################
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |

# pound
less             6 0 8
greater          6 0 1
bar              6 0 8
brokenbar        6 0 8
# *
#plus             6 1 8
#asterisk         6 1 1
# semi-colon
adiaeresis       6 2 8
Adiaeresis       6 2 1
# extra: altgr+] -> ;+shift
bracketright     6 2 1
# clr/home
Home             6 3 8
# extra: altgr+\ -> clr/home
backslash        6 3 8
# right shift
# key is right shift
Shift_R          6 4 4
# =
apostrophe       6 5 8
asterisk         6 5 8
# arrow up / pi
End              6 6 8
# extra: altgr+~ -> arrow up
asciitilde       6 6 8
# extra: altgr+m -> arrow up+shift (pi)
mu               6 6 1
# / ?
minus            6 7 8
underscore       6 7 1

#####################
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |

# shift+1
exclam           7 0 8
# left arrow
section          7 1 8
degree           7 1 8
# ctrl
#Tab            7 2 8+16384  key is CTRL
Tab            7 2 16392
#ISO_Left_Tab   7 2 16384+8  key is CTRL
ISO_Left_Tab   7 2 16392
# shift+2
quotedbl         7 3 8
# space
space            7 4 8
# cbm
#Control_L        7 5 8+8192  key is CBM
Control_L        7 5 8200
# run/stop
Escape           7 7 8

#####################
# letters and numbers

0 4 3 8
1 7 0 8
2 7 3 8
3 1 0 8
4 1 3 8
5 2 0 8
6 2 3 8
7 3 0 8
8 3 3 8
9 4 0 8

A 1 2 8
B 3 4 8
C 2 4 8
D 2 2 8
E 1 6 8
F 2 5 8
G 3 2 8
H 3 5 8
I 4 1 8
J 4 2 8
K 4 5 8
L 5 2 8
M 4 4 8
N 4 7 8
O 4 6 8
P 5 1 8
Q 7 6 8
R 2 1 8
S 1 5 8
T 2 6 8
U 3 6 8
V 3 7 8
W 1 1 8
X 2 7 8
Y 3 1 8
Z 1 4 8
a 1 2 8
b 3 4 8
c 2 4 8
d 2 2 8
e 1 6 8
f 2 5 8
g 3 2 8
h 3 5 8
i 4 1 8
j 4 2 8
k 4 5 8
l 5 2 8
m 4 4 8
n 4 7 8
o 4 6 8
p 5 1 8
q 7 6 8
r 2 1 8
s 1 5 8
t 2 6 8
u 3 6 8
v 3 7 8
w 1 1 8
x 2 7 8
z 1 4 8
y 3 1 8

#
# Restore key mappings
#
F12 -3 0
F12 -3 1

# Dead keys support
dead_acute      5 3 8  # ' -> pound
dead_grave      5 3 8  # ` -> shift+pound
dead_diaeresis  6 1 8  # ¨ -> asterisk
dead_circumflex 6 1 8  # ^ -> shift+asterisk

#
# joyport attached keypad
#
Num_Lock    -5 0
KP_7        -5 1
KP_8        -5 2
KP_9        -5 3
KP_Divide   -5 4
Scroll_Lock -5 5
KP_4        -5 6
KP_5        -5 7
KP_6        -5 8
KP_Multiply -5 9
Sys_Req     -5 10
KP_1        -5 11
KP_2        -5 12
KP_3        -5 13
KP_Subtract -5 14
Print       -5 15
KP_0        -5 16
KP_Delete   -5 17
KP_Enter    -5 18
KP_Add      -5 19
