# VICE keyboard mapping file
#
# A Keyboard map is read in as patch to the current map.
#
# File format:
# - comment lines start with '#'
# - keyword lines start with '!keyword'
# - normal line has 'keysym/scancode row column shiftflag'
#
# Keywords and their lines are:
# '!CLEAR'               clear whole table
# '!INCLUDE filename'    read file as mapping file
# '!LSHIFT row col'      left shift keyboard row/column
# '!RSHIFT row col'      right shift keyboard row/column
# '!VSHIFT shiftkey'     virtual shift key (RSHIFT or LSHIFT)
# '!SHIFTL shiftkey'     shift lock key (RSHIFT or LSHIFT)
# '!UNDEF keysym'        remove keysym from table
#
# Shiftflag can have the values:
# 0      key is not shifted for this keysym/scancode
# 1      key is shifted for this keysym/scancode
# 2      left shift
# 4      right shift
# 8      key can be shifted or not with this keysym/scancode
# 16     deshift key for this keysym/scancode
# 32     another definition for this keysym/scancode follows
# 64     shift lock
# 256    key is used for an alternative keyboard mapping
#
# Negative row values:
# 'keysym -1 n' joystick keymap A, direction n
# 'keysym -2 n' joystick keymap B, direction n
# 'keysym -3 0' first RESTORE key
# 'keysym -3 1' second RESTORE key
# 'keysym -4 0' 40/80 column key
# 'keysym -4 1' CAPS (ASCII/DIN) key
# 'keysym -5 n' joyport keypad, key n
#
# Joystick direction values:
# 0      Fire
# 1      South/West
# 2      South
# 3      South/East
# 4      West
# 5      East
# 6      North/West
# 7      North
# 8      North/East
#
# Joyport keypad key layout:
# --------------------------
# |  0 |  1 |  2 |  3 |  4 |
# --------------------------
# |  5 |  6 |  7 |  8 |  9 |
# --------------------------
# | 10 | 11 | 12 | 13 | 14 |
# --------------------------
# | 15 | 16 | 17 | 18 | 19 |
# --------------------------
#
# When a bigger spaced key is used,
# it uses the upper left most key value.

# Symbolic Mapping, Danish Layout, C64, GTK3

# C64 keyboard matrix:
#
#       +-----+-----+-----+-----+-----+-----+-----+-----+
#       |Bit 0|Bit 1|Bit 2|Bit 3|Bit 4|Bit 5|Bit 6|Bit 7|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+

!CLEAR
!LSHIFT 1 7
!RSHIFT 6 4
!VSHIFT RSHIFT
!SHIFTL LSHIFT

#####################
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|

BackSpace       0 0 8
Delete          0 0 8
Insert          0 0 16
Return          0 1 8
Right           0 2 8
KP_F4           0 2 8
Left            0 2 1
F7              0 3 8
F8              0 3 1
F1              0 4 8
KP_F1           0 4 8
F2              0 4 1
KP_F2           0 5 8
F3              0 5 8
F4              0 5 1
F5              0 6 8
KP_F3           0 6 8
F6              0 6 1
Down            0 7 8
Up              0 7 1

#####################
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |

numbersign      1 0 1
dollar          1 3 1
currency        1 3 1   /* da-fix - enable $ instead of ¤ */
Shift_L         1 7 2
# shift lock
Caps_Lock       1 7 64

#####################
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |

percent         2 0 1
ampersand       2 3 1

#####################
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |

apostrophe      3 0 1
parenleft       3 3 1

#####################
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |

parenright      4 0 1

#####################
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |

plus            5 0 0
minus           5 3 0
period          5 4 0
greater         5 4 1
colon           5 5 0
ae              5 5 1
aring           5 6 0
comma           5 7 0
less            5 7 1

#####################
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |

dead_acute      6 0 0
dead_grave      6 0 1
asterisk        6 1 0
semicolon       6 2 0
oslash          6 2 1
Home            6 3 8
Shift_R         6 4 4
equal           6 5 0
dead_circumflex 6 6 1
dead_diaeresis  6 6 0
slash           6 7 0
question        6 7 1

#####################
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |

exclam          7 0 1
underscore      7 1 0
onehalf         7 1 0
Tab             7 2 8     /* Tab = CTRL */
ISO_Left_Tab    7 2 8     /* Shift + Tab = CTRL */
quotedbl        7 3 1
space           7 4 8
Control_L       7 5 8     /* Control_L = CBM */
Escape          7 7 8

#####################
# letters and numbers

0 4 3 0
1 7 0 0
2 7 3 0
3 1 0 0
4 1 3 0
5 2 0 0
6 2 3 0
7 3 0 0
8 3 3 0
9 4 0 0

A 1 2 1
B 3 4 1
C 2 4 1
D 2 2 1
E 1 6 1
F 2 5 1
G 3 2 1
H 3 5 1
I 4 1 1
J 4 2 1
K 4 5 1
L 5 2 1
M 4 4 1
N 4 7 1
O 4 6 1
P 5 1 1
Q 7 6 1
R 2 1 1
S 1 5 1
T 2 6 1
U 3 6 1
V 3 7 1
W 1 1 1
X 2 7 1
Y 3 1 1
Z 1 4 1
a 1 2 8
b 3 4 8
c 2 4 8
d 2 2 8
e 1 6 8
f 2 5 8
g 3 2 8
h 3 5 8
i 4 1 8
j 4 2 8
k 4 5 8
l 5 2 8
m 4 4 8
n 4 7 8
o 4 6 8
p 5 1 8
q 7 6 8
r 2 1 8
s 1 5 8
t 2 6 8
u 3 6 8
v 3 7 8
w 1 1 8
x 2 7 8
y 3 1 8
z 1 4 8

# Restore key mappings
Page_Up -3 0
Prior -3 1

#
# joyport attached keypad
#
Num_Lock    -5 0
KP_7        -5 1
KP_8        -5 2
KP_9        -5 3
KP_Divide   -5 4
Scroll_Lock -5 5
KP_4        -5 6
KP_5        -5 7
KP_6        -5 8
KP_Multiply -5 9
Sys_Req     -5 10
KP_1        -5 11
KP_2        -5 12
KP_3        -5 13
KP_Subtract -5 14
Print       -5 15
KP_0        -5 16
KP_Delete   -5 17
KP_Enter    -5 18
KP_Add      -5 19
